# Example PlatformIO Project Configuration Override
# ------------------------------------------------------------------------------
# Copy to platformio_override.ini to activate overrides
# ------------------------------------------------------------------------------
# Please visit documentation: https://docs.platformio.org/page/projectconf.html

[env:esp8266_1m_custom]
board = esp01_1m
platform = ${common.arduino_core_2_4_2}
board_build.ldscript = ${common.ldscript_1m0m}
build_flags = ${common.build_flags_esp8266} 
  -D WLED_DISABLE_OTA 
  -D WLED_DISABLE_ALEXA 
  -D WLED_DISABLE_BLYNK
  -D WLED_DISABLE_CRONIXIE 
  -D WLED_DISABLE_HUESYNC 
  -D WLED_DISABLE_INFRARED
; PIN defines - uncomment and change, if needed:
;   -D LEDPIN=2
;   -D BTNPIN=0
;   -D IR_PIN=4
;   -D RLYPIN=12
;   -D RLYMDE=1
; digital LED strip types - uncomment only one ! - this will disable WS281x / SK681x support
;   -D USE_APA102
;   -D USE_WS2801
;   -D USE_LPD8806
; to drive analog LED strips (aka 5050), uncomment the following
; PWM pins 5,12,13,15 are used with Magic Home LED Controller (default)
;   -D WLED_USE_ANALOG_LEDS
; for the H801 controller (PINs 15,13,12,14 (W2 = 04)) uncomment this
;   -D WLED_USE_H801
; for the BW-LT11 controller (PINs 12,4,14,5 ) uncomment this
;   -D WLED_USE_BWLT11
; and to enable channel 5 for RGBW-CT led strips this
;   -D WLED_USE_5CH_LEDS
