# LED Settings

## LED setup

LED count:
⚠ You might run into stability or lag issues.
Use less than 1000 LEDs per ESP for the best experience!
Recommended power supply for brightest white:
?
Enable automatic brightness limiter:
Maximum Current: mA
⚠ Your power supply provides high current.
To improve the safety of your setup,
please use thick cables,
multiple power injection points and a fuse!
Automatically limits brightness to stay close to the limit.
Keep at <1A if powering LEDs directly from the ESP 5V pin!
If you are using an external power supply, enter its rating.
(Current estimated usage: unknown)
LED voltage (Max. current for a single LED):
Custom max. current per LED: mA
Keep at default if you are unsure about your type of LEDs.
LEDs are 4-channel type (RGBW):
Auto-calculate white channel from RGB:
Color order:

### Defaults

Turn LEDs on after power up/reset:
Default brightness: (0-255)
Apply preset at boot (0 uses defaults)
- or -
Set current preset cycle setting as boot default:
Use Gamma correction for color: (strongly recommended)
Use Gamma correction for brightness: (not recommended)
Brightness factor: %

### Transitions

Crossfade:
Transition Time: ms
Enable Palette transitions:

### Timed light

Default Duration: min
Default Target brightness:
Fade down:

### Advanced

Palette blending:
Reverse LED order (rotate 180):
Skip first LED: