# Misc Settings

## Security & Update setup

Lock wireless (OTA) software update:
Passphrase:
To enable OTA, for security reasons you need to also enter the correct password!
The password should be changed when OTA is enabled.
Disable OTA when not in use, otherwise an attacker can reflash device software!
Settings on this page are only changable if OTA lock is disabled!
Deny access to WiFi settings if locked:
Factory reset:
All EEPROM content (settings) will be erased.
HTTP traffic is unencrypted. An attacker in the same network can intercept form data!

### Software Update

Enable ArduinoOTA:

### About

WLED version 0.10.0
Contributors, dependencies and special thanks
A huge thank you to everyone who helped me create WLED!
(c) 2016-2019 Christian Schwinne
Licensed under the MIT license
Server message: Response error!